| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
fds_ic_t Struct Reference
Flash Data Storage

Part of the record metadata. More...

`#include <fds.h>`

## Data Fields
uint16_t | file_id
| The ID of the file that the record belongs to.
uint16_t | crc16
| CRC16 check value. More...

## Detailed Description

Part of the record metadata.

Contains the ID of the file that the record belongs to and the CRC16 check value of the record.

## Field Documentation

uint16_t fds_ic_t::crc16

CRC16 check value.

The CRC is calculated over the entire record as stored in flash (including the record metadata except the CRC field itself). The CRC standard employed is CRC-16-CCITT.