| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Enumerations
Enumerations
Battery Service Client

## Enumerations
enum | ble_bas_c_evt_type_t { BLE_BAS_C_EVT_DISCOVERY_COMPLETE, BLE_BAS_C_EVT_BATT_NOTIFICATION, BLE_BAS_C_EVT_BATT_READ_RESP }
| Battery Service Client event type. More...

## Detailed Description

## Enumeration Type Documentation

enum ble_bas_c_evt_type_t

Battery Service Client event type.

Enumerator
BLE_BAS_C_EVT_DISCOVERY_COMPLETE | Event indicating that the Battery Service has been discovered at the peer.
BLE_BAS_C_EVT_BATT_NOTIFICATION | Event indicating that a notification of the Battery Level characteristic has been received from the peer.
BLE_BAS_C_EVT_BATT_READ_RESP | Event indicating that a read response on Battery Level characteristic has been received from peer.