| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_ble_bms_features_t Struct Reference
Bond Management Service

Supported features. More...

`#include <nrf_ble_bms.h>`

## Data Fields
bool | delete_all: 1
| Indicates whether the application wants to support the operation to delete all bonds.
bool | delete_all_auth: 1
| Indicates whether the application wants to support the operation to delete all bonds with authorization code.
bool | delete_requesting: 1
| Indicates whether the application wants to support the operation to delete the bonds of the requesting device.
bool | delete_requesting_auth: 1
| Indicates whether the application wants to support the operation to delete the bonds of the requesting device with authorization code.
bool | delete_all_but_requesting: 1
| Indicates whether the application wants to support the operation to delete all bonds except for the bond of the requesting device.
bool | delete_all_but_requesting_auth: 1
| Indicates whether the application wants to support the operation to delete all bonds except for the bond of the requesting device with authorization code.

## Detailed Description

Supported features.