| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
ANT common search configuration configuration
ANT search configuration

## Macros
#define | ANT_SEARCH_CONFIG_ENABLED
| Enable ANT common search configuration. * Set to 1 to activate. More...
#define | ANT_DEFAULT_LOW_PRIORITY_TIMEOUT
| Default low priority search time-out. * Minimum value: 0 Maximum value: 255. More...
#define | ANT_DEFAULT_HIGH_PRIORITY_TIMEOUT
| Default high priority search time-out. * Minimum value: 0 Maximum value: 255. More...

## Detailed Description

## Macro Definition Documentation

#define ANT_DEFAULT_HIGH_PRIORITY_TIMEOUT

Default high priority search time-out. * Minimum value: 0 Maximum value: 255.

Note
  This is an NRF_CONFIG macro.

#define ANT_DEFAULT_LOW_PRIORITY_TIMEOUT

Default low priority search time-out. * Minimum value: 0 Maximum value: 255.

Note
  This is an NRF_CONFIG macro.

#define ANT_SEARCH_CONFIG_ENABLED

Enable ANT common search configuration. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.