| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
pm_peer_data_update_succeeded_evt_t Struct Reference
Peer Manager

Parameters specific to the PM_EVT_PEER_DATA_UPDATE_SUCCEEDED event. More...

`#include <peer_manager.h>`

## Data Fields
pm_peer_data_id_t | data_id
| The type of the data that was changed.
pm_peer_data_op_t | action
| What happened to the data.
uint8_t | flash_changed: 1
| If this is false, no operation was done in flash, because the value was already what it should be. Please note that in certain scenarios, this flag will be true even if the new value is the same as the old.
pm_store_token_t | token
| Token that identifies the operation. For PM_PEER_DATA_OP_DELETE actions, this token can be disregarded. For PM_PEER_DATA_OP_UPDATE actions, compare this token with the token that is received from a call to a PM_PEER_DATA_FUNCTIONS function.

## Detailed Description

Parameters specific to the PM_EVT_PEER_DATA_UPDATE_SUCCEEDED event.