| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ant_encrypt_stack_settings_t Struct Reference
ANT encryption configuration

ANT stack cryptographic configuration. More...

`#include <ant_encrypt_config.h>`

## Data Fields
ant_encrypt_info_settings_t | info
| Pointer to the encryption information structure.
uint8_t ** | pp_key
| Pointer to an array for pointers to encryption keys. Each key must have a length of 16 bytes.
uint8_t | key_number
| Number of encryption keys.
ant_encrypt_adv_burst_settings_t * | p_adv_burst_config
| Advanced burst configuration. If NULL, the advanced burst must be configured externally.

## Detailed Description

ANT stack cryptographic configuration.