| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ancs_c_notif_flags_t Struct Reference
Apple Notification Service client

Flags for iOS notifications. More...

`#include <ble_ancs_c.h>`

## Data Fields
uint8_t | silent: 1
uint8_t | important: 1
uint8_t | pre_existing: 1
uint8_t | positive_action: 1
uint8_t | negative_action: 1

## Detailed Description

Flags for iOS notifications.

## Field Documentation

uint8_t ble_ancs_c_notif_flags_t::important

If this flag is set, the notification has a high priority.

uint8_t ble_ancs_c_notif_flags_t::negative_action

If this flag is set, the notification has a negative action that can be taken.

uint8_t ble_ancs_c_notif_flags_t::positive_action

If this flag is set, the notification has a positive action that can be taken.

uint8_t ble_ancs_c_notif_flags_t::pre_existing

If this flag is set, the notification is pre-existing.

uint8_t ble_ancs_c_notif_flags_t::silent

If this flag is set, the notification has a low priority.