| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
DFU bootloader examples

You can use a Device Firmware Update (DFU) to update the SoftDevice, bootloader, or application on an nRF5 SoC over-the-air (OTA).

See the following example if you use the ANT protocol and the ANT-FS transport:

- Experimental: ANT Bootloader/DFU

See the following examples if you use BLE transport:

- BLE Secure DFU Bootloader
- Experimental: Buttonless DFU Template Application