| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_bps_init_t Struct Reference
Blood Pressure Service

Blood Pressure Service init structure. This contains all options and data needed for initialization of the service. More...

`#include <ble_bps.h>`

## Data Fields
ble_bps_evt_handler_t | evt_handler
ble_srv_cccd_security_mode_t | bps_meas_attr_md
ble_srv_security_mode_t | bps_feature_attr_md
uint16_t | feature

## Detailed Description

Blood Pressure Service init structure. This contains all options and data needed for initialization of the service.

## Field Documentation

ble_srv_security_mode_t ble_bps_init_t::bps_feature_attr_md

Initial security level for blood pressure feature attribute

ble_srv_cccd_security_mode_t ble_bps_init_t::bps_meas_attr_md

Initial security level for blood pressure measurement attribute

ble_bps_evt_handler_t ble_bps_init_t::evt_handler

Event handler to be called for handling events in the Blood Pressure Service.

uint16_t ble_bps_init_t::feature

Initial value for blood pressure feature