| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gattc_write_params_t Struct Reference
Structures

Write Parameters. More...

`#include <ble_gattc.h>`

## Data Fields
uint8_t | write_op
uint8_t | flags
uint16_t | handle
uint16_t | offset
uint16_t | len
uint8_t const * | p_value

## Detailed Description

Write Parameters.

## Field Documentation

uint8_t ble_gattc_write_params_t::flags

Flags, see GATT Execute Write flags.

uint16_t ble_gattc_write_params_t::handle

Handle to the attribute to be written.

uint16_t ble_gattc_write_params_t::len

Length of data in bytes.

uint16_t ble_gattc_write_params_t::offset

Offset in bytes.

Note
  For WRITE_CMD and WRITE_REQ, offset must be 0.

uint8_t const* ble_gattc_write_params_t::p_value

Pointer to the value data.

uint8_t ble_gattc_write_params_t::write_op

Write Operation to be performed, see GATT Write operations.