| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Vendor Specific UUID counts
Defines

## Macros
#define | BLE_UUID_VS_COUNT_MIN 1
#define | BLE_UUID_VS_COUNT_DEFAULT 0

## Detailed Description

## Macro Definition Documentation

#define BLE_UUID_VS_COUNT_DEFAULT 0

Use the default VS UUID count (10 for this version of the SoftDevice).

#define BLE_UUID_VS_COUNT_MIN 1

Minimum VS UUID count.