| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_sec_keys_t Struct Reference
Structures

Security Keys. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_enc_key_t * | p_enc_key
ble_gap_id_key_t * | p_id_key
ble_gap_sign_info_t * | p_sign_key
ble_gap_lesc_p256_pk_t * | p_pk

## Detailed Description

Security Keys.

## Field Documentation

ble_gap_enc_key_t* ble_gap_sec_keys_t::p_enc_key

Encryption Key, or NULL.

ble_gap_id_key_t* ble_gap_sec_keys_t::p_id_key

Identity Key, or NULL.

ble_gap_lesc_p256_pk_t* ble_gap_sec_keys_t::p_pk

                   LE Secure Connections P-256 Public Key. When in debug mode the application must use the value defined

in the Core Bluetooth Specification v4.2 Vol.3, Part H, Section 2.3.5.6.1

ble_gap_sign_info_t* ble_gap_sec_keys_t::p_sign_key

Signing Key, or NULL.