| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ieee_float16_t Struct Reference
Blood Pressure Service

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit vlue with 12-bit mantissa and 4-bit exponent. More...

`#include <ble_bps.h>`

## Data Fields
int8_t | exponent
int16_t | mantissa

## Detailed Description

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit vlue with 12-bit mantissa and 4-bit exponent.

## Field Documentation

int8_t ieee_float16_t::exponent

Base 10 exponent, only 4 bits

int16_t ieee_float16_t::mantissa

Mantissa, only 12 bits