| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatt_char_props_t Struct Reference
Structures

GATT Characteristic Properties. More...

`#include <ble_gatt.h>`

## Data Fields
uint8_t | broadcast:1
uint8_t | read:1
uint8_t | write_wo_resp:1
uint8_t | write:1
uint8_t | notify:1
uint8_t | indicate:1
uint8_t | auth_signed_wr:1

## Detailed Description

GATT Characteristic Properties.

## Field Documentation

uint8_t ble_gatt_char_props_t::auth_signed_wr

Writing the value with Signed Write Command permitted.

uint8_t ble_gatt_char_props_t::broadcast

Broadcasting of the value permitted.

uint8_t ble_gatt_char_props_t::indicate

Indications of the value permitted.

uint8_t ble_gatt_char_props_t::notify

Notications of the value permitted.

uint8_t ble_gatt_char_props_t::read

Reading the value permitted.

uint8_t ble_gatt_char_props_t::write

Writing the value with Write Request permitted.

uint8_t ble_gatt_char_props_t::write_wo_resp

Writing the value with Write Command permitted.