| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
pm_conn_sec_status_t Struct Reference
Peer Manager

Security status of a connection. More...

`#include <peer_manager.h>`

## Data Fields
uint8_t | connected: 1
| The connection is active (not disconnected).
uint8_t | encrypted: 1
| Communication on this link is encrypted.
uint8_t | mitm_protected: 1
| The encrypted communication is also protected against man-in-the-middle attacks.
uint8_t | bonded: 1
| The peer is bonded with us.

## Detailed Description

Security status of a connection.