| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Advertising timeout values
Defines

## Macros
#define | BLE_GAP_ADV_TIMEOUT_LIMITED_MAX (180)
#define | BLE_GAP_ADV_TIMEOUT_GENERAL_UNLIMITED (0)

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADV_TIMEOUT_GENERAL_UNLIMITED (0)

Unlimited advertising in general discoverable mode.

#define BLE_GAP_ADV_TIMEOUT_LIMITED_MAX (180)

Maximum advertising time in limited discoverable mode (TGAP(lim_adv_timeout) = 180s).