| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_common_evt_t Struct Reference
Structures

Event structure for events not associated with a specific function module. More...

`#include <ble.h>`

## Data Fields
uint16_t | conn_handle
union {
ble_evt_tx_complete_t tx_complete
ble_evt_user_mem_request_t user_mem_request
ble_evt_user_mem_release_t user_mem_release
ble_evt_data_length_changed_t data_length_changed
} | params

## Detailed Description

Event structure for events not associated with a specific function module.

## Field Documentation

uint16_t ble_common_evt_t::conn_handle

Connection Handle on which this event occurred.

ble_evt_data_length_changed_t ble_common_evt_t::data_length_changed

Data Length Changed Event Parameters.

union { ... } ble_common_evt_t::params

Event parameter union.

ble_evt_tx_complete_t ble_common_evt_t::tx_complete

Transmission Complete.

ble_evt_user_mem_release_t ble_common_evt_t::user_mem_release

User Memory Release Event Parameters.

ble_evt_user_mem_request_t ble_common_evt_t::user_mem_request

User Memory Request Event Parameters.