| S212 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ANT_HIGH_DUTY_SEARCH_CONFIG Struct Reference
ANT Stack Parameters

Used with the get/set high duty search config commands. More...

`#include <ant_parameters.h>`

## Data Fields
uint8_t | bEnable
| Enable or disable high duty search. See HIGH_DUTY_SEARCH defines in ant_parameters.h.
uint8_t | ucSearchSuppressionWindows
| Number of windows to apply suppression for. See HIGH_DUTY_SEARCH defines in ant_parameters.h.
uint16_t | usRestartInterval
| Restart interval is reset back to default when high duty search is disabled. More...

## Detailed Description

Used with the get/set high duty search config commands.

## Field Documentation

uint16_t ANT_HIGH_DUTY_SEARCH_CONFIG::usRestartInterval

Restart interval is reset back to default when high duty search is disabled.

Restart interval. Use default value of HIGH_DUTY_SEARCH_RESTART_INTERVAL_DEFAULT unless otherwise specified. See HIGH_DUTY_SEARCH defines in ant_parameters.h