| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_sec_keyset_t Struct Reference
Structures

Security key set for both local and peer keys. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_sec_keys_t | keys_own
ble_gap_sec_keys_t | keys_peer

## Detailed Description

Security key set for both local and peer keys.

## Field Documentation

ble_gap_sec_keys_t ble_gap_sec_keyset_t::keys_own

Keys distributed by the local device. For LE Secure Connections the encryption key will be generated locally and will always be stored if bonding.

ble_gap_sec_keys_t ble_gap_sec_keyset_t::keys_peer

Keys distributed by the remote device. For LE Secure Connections, p_enc_key must always be NULL.