| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Clock accuracy
Defines

## Macros
#define | NRF_CLOCK_LF_XTAL_ACCURACY_250_PPM (0)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_500_PPM (1)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_150_PPM (2)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_100_PPM (3)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_75_PPM (4)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_50_PPM (5)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_30_PPM (6)
#define | NRF_CLOCK_LF_XTAL_ACCURACY_20_PPM (7)

## Detailed Description

## Macro Definition Documentation

#define NRF_CLOCK_LF_XTAL_ACCURACY_100_PPM (3)

100 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_150_PPM (2)

150 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_20_PPM (7)

20 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_250_PPM (0)

Default: 250 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_30_PPM (6)

30 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_500_PPM (1)

500 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_50_PPM (5)

50 ppm

#define NRF_CLOCK_LF_XTAL_ACCURACY_75_PPM (4)

75 ppm