| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ant_bsc_profile_s Struct Reference
Bicycle Speed and Cadence profile

BSC profile structure. More...

`#include <ant_bsc.h>`

## Data Fields
uint8_t | channel_number
| Channel number assigned to the profile.
union {
ant_bsc_disp_cb_t * p_disp_cb
ant_bsc_sens_cb_t * p_sens_cb
} | _cb
| Pointer to internal control block.
ant_bsc_evt_handler_t | evt_handler
| Event handler to be called for handling events in the BSC profile.
ant_bsc_page0_data_t | page_0
| Page 0.
ant_bsc_page1_data_t | page_1
| Page 1.
ant_bsc_page2_data_t | page_2
| Page 2.
ant_bsc_page3_data_t | page_3
| Page 3.
ant_bsc_page4_data_t | page_4
| Page 4.
ant_bsc_page5_data_t | page_5
| Page 5.
ant_bsc_combined_page0_data_t | page_comb_0
| Page 0 for combined speed and cadence sensor.

## Detailed Description

BSC profile structure.