| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
type_2_tag_serial_number_t Struct Reference
Type 2 Tag

Descriptor for the internal bytes of a Type 2 Tag. More...

`#include <nfc_t2t_parser.h>`

## Data Fields
uint8_t | manufacturer_id
| Manufacturer ID (the most significant byte of the UID/serial number).
uint16_t | serial_number_part_1
| Bytes 5-4 of the tag UID.
uint8_t | check_byte_0
| First block check character byte (XOR of the cascade tag byte, manufacturer ID byte, and the serial_number_part_1 bytes).
uint32_t | serial_number_part_2
| Bytes 3-0 of the tag UID.
uint8_t | check_byte_1
| Second block check character byte (XOR of the serial_number_part_2 bytes).
uint8_t | internal
| Tag internal bytes.

## Detailed Description

Descriptor for the internal bytes of a Type 2 Tag.