| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
type_2_tag_t Struct Reference
Type 2 Tag

Type 2 Tag descriptor. More...

`#include <nfc_t2t_parser.h>`

## Data Fields
type_2_tag_serial_number_t | sn
| Values within the serial number area of the tag.
uint16_t | lock_bytes
| Value of the lock bytes.
type_2_tag_capability_container_t | cc
| Values within the Capability Container area of the tag.
uint16_t const | max_tlv_blocks
| Maximum number of TLV blocks that can be stored.
tlv_block_t * | p_tlv_block_array
| Pointer to the array for TLV blocks.
uint16_t | tlv_count
| Number of TLV blocks stored in the Type 2 Tag.

## Detailed Description

Type 2 Tag descriptor.