| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules | Macros
Defines
Generic Attribute Profile (GATT) Common

## Modules
| Characteristic Presentation Formats
| GATT Bluetooth Namespaces
| GATT Execute Write flags
| GATT Handle Value operations
| GATT Status Codes
| GATT Timeout sources
| GATT Write operations

## Macros
#define | GATT_MTU_SIZE_DEFAULT 23
| Default MTU size, in bytes.
#define | BLE_GATT_HANDLE_INVALID 0x0000
| Invalid Attribute Handle.
#define | BLE_GATT_HANDLE_START 0x0001
| First Attribute Handle.
#define | BLE_GATT_HANDLE_END 0xFFFF
| Last Attribute Handle.

## Detailed Description