| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_sec_request_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_SEC_REQUEST. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | bond: 1
uint8_t | mitm: 1
uint8_t | lesc: 1
uint8_t | keypress: 1

## Detailed Description

Event structure for BLE_GAP_EVT_SEC_REQUEST.

## Field Documentation

uint8_t ble_gap_evt_sec_request_t::bond

Perform bonding.

uint8_t ble_gap_evt_sec_request_t::keypress

Generation of keypress notifications requested.

uint8_t ble_gap_evt_sec_request_t::lesc

LE Secure Connections requested.

uint8_t ble_gap_evt_sec_request_t::mitm

Man In The Middle protection requested.